| OrbbecSDK 1.10.18 OrbbecSDK: Software-Development-Kit for Orbbec 3D Cameras

Loading...
Searching...
No Matches
Public Attributes | List of all members
OBNetIpConfig Struct Reference

IP address configuration for network devices (IPv4) More...

`#include <ObTypes.h>`

## Public Attributes
uint16_t | dhcp
| DHCP status.
uint8_t | address [4]
| IP address (IPv4, big endian: 192.168.1.10, address[0] = 192, address[1] = 168, address[2] = 1, address[3] = 10)
uint8_t | mask [4]
| Subnet mask (big endian)
uint8_t | gateway [4]
| Gateway (big endian)

## Detailed Description

IP address configuration for network devices (IPv4)

Definition at line 1121 of file ObTypes.h.

## Member Data Documentation

## ◆ dhcp

uint16_t OBNetIpConfig::dhcp

DHCP status.

Note
  0: static IP; 1: DHCP

Definition at line 1127 of file ObTypes.h.

## ◆ address

uint8_t OBNetIpConfig::address[4]

IP address (IPv4, big endian: 192.168.1.10, address[0] = 192, address[1] = 168, address[2] = 1, address[3] = 10)

Definition at line 1132 of file ObTypes.h.

## ◆ mask

uint8_t OBNetIpConfig::mask[4]

Subnet mask (big endian)

Definition at line 1137 of file ObTypes.h.

## ◆ gateway

uint8_t OBNetIpConfig::gateway[4]

Gateway (big endian)

Definition at line 1142 of file ObTypes.h.

The documentation for this struct was generated from the following file:

- E:/Projects/Jenkins/workspace/OrbbecSDK/libobsensor/include/libobsensor/h/ObTypes.h