| aiengine Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

xaiegbl_g.c File Reference

## Overview

This file contains a configuration table that specifies the configuration of AIE devices in the system.

    MODIFICATION HISTORY:

    Ver   Who     Date     Changes

    1.0  Naresh  03/14/2018  Initial creation
    1.1  Naresh  07/11/2018  Updated copyright info
    1.2  Nishad  12/05/2018  Renamed ME attributes to AIE

## Variables
XAieGbl_Config | XAieGbl_ConfigTable [XPAR_AIE_NUM_INSTANCES]
| The configuration table for each AIE device. More...

## Variable Documentation

XAieGbl_Config XAieGbl_ConfigTable[XPAR_AIE_NUM_INSTANCES]

Initial value:
=
{
{
XPAR_AIE_DEVICE_ID,
XPAR_AIE_ARRAY_OFFSET,
XPAR_AIE_NUM_ROWS,
XPAR_AIE_NUM_COLUMNS
}
}

The configuration table for each AIE device.

XAIE_BASE_ARRAY_ADDR_OFFSET macro defines the AI Engine's base address offset value.