| rfdc Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xrfdc_mts.c File Reference

## Functions
u32 | XRFdc_MTS_Sysref_Config (XRFdc *InstancePtr, XRFdc_MultiConverter_Sync_Config *DACSyncConfigPtr, XRFdc_MultiConverter_Sync_Config *ADCSyncConfigPtr, u32 SysRefEnable)
| This API is used to enable/disable the sysref. More...
u32 | XRFdc_MultiConverter_Init (XRFdc_MultiConverter_Sync_Config *ConfigPtr, int *PLL_CodesPtr, int *T1_CodesPtr, u32 RefTile)
| This API Initializes the multi-tile sync config structures. More...
u32 | XRFdc_MultiConverter_Sync (XRFdc *InstancePtr, u32 Type, XRFdc_MultiConverter_Sync_Config *ConfigPtr)
| This is the top level API which will be used for Multi-tile Synchronization. More...
u32 | XRFdc_GetMTSEnable (XRFdc *InstancePtr, u32 Type, u32 Tile_Id, u32 *EnablePtr)
| This is the top level API which will be used to check if Multi-tile is enabled. More...
u32 | XRFdc_GetMasterTile (XRFdc *InstancePtr, u32 Type)
| Get Master Tile for ADC/DAC tiles. More...
u32 | XRFdc_GetSysRefSource (XRFdc *InstancePtr, u32 Type)
| Get Sysref source for ADC/DAC tile. More...