| dfeccf Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeCcf_TriggerCfg Struct Reference
Overview

All IP triggers. More...

## Data Fields
XDfeCcf_Trigger | Activate
                       Switch between "Initialized",
ultra-low power state, and "Operational". More...
XDfeCcf_Trigger | LowPower
                       Switch between "Low-power"
and "Operational" state. More...
XDfeCcf_Trigger | CCUpdate
                       Transition to next CC
configuration. More...
XDfeCcf_Trigger | Switch
                     Switch between Downlink and Uplink datapth
configuration. More...

## Detailed Description

All IP triggers.

## Field Documentation

XDfeCcf_Trigger XDfeCcf_TriggerCfg::Activate

                       Switch between "Initialized",

ultra-low power state, and "Operational".

One-shot trigger, disabled following a single event.

Referenced by XDfeCcf_GetTriggersCfg(), XDfeCcf_PassThroughExample(), and XDfeCcf_SetTriggersCfg().

XDfeCcf_Trigger XDfeCcf_TriggerCfg::CCUpdate

                       Transition to next CC

configuration.

Will initiate flush based on CC configuration.

Referenced by XDfeCcf_GetTriggersCfg(), XDfeCcf_PassThroughExample(), and XDfeCcf_SetTriggersCfg().

XDfeCcf_Trigger XDfeCcf_TriggerCfg::LowPower

                       Switch between "Low-power"

and "Operational" state.

Referenced by XDfeCcf_GetTriggersCfg(), and XDfeCcf_SetTriggersCfg().

XDfeCcf_Trigger XDfeCcf_TriggerCfg::Switch

                     Switch between Downlink and Uplink datapth

configuration.

Will initiate flush based on CC configuration.

Referenced by XDfeCcf_GetTriggersCfg(), and XDfeCcf_SetTriggersCfg().