| dfeprach Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfePrach_MixerStatusOverflow Struct Reference
Overview

PRACH status. More...

## Data Fields
u32 | MixerOverflow
                [0-1] Source of first occurrence of overflow
as signalled in ISR. More...
u32 | FirstAntennaOverflowing
                          [0-7] Lowest numbered antenna on
which first mixer overflow occurred. More...
u32 | FirstRCIdOverflowing
                       [0-15] The physical mixer on which
the first mixer overflow occurred. More...

## Detailed Description

PRACH status.

## Field Documentation

u32 XDfePrach_MixerStatusOverflow::FirstAntennaOverflowing

                          [0-7] Lowest numbered antenna on

which first mixer overflow occurred.

Referenced by XDfePrach_GetStatus().

u32 XDfePrach_MixerStatusOverflow::FirstRCIdOverflowing

                       [0-15] The physical mixer on which

the first mixer overflow occurred.

Each mixer handles 4 rach channels, and the overflow indicator is agregated, so an overflow on physical channel 0-3 will indicate as an overflow on Channel 0, 4-7: channel 1, etc.

Referenced by XDfePrach_GetStatus().

u32 XDfePrach_MixerStatusOverflow::MixerOverflow

                [0-1] Source of first occurrence of overflow

as signalled in ISR.

That is, register only updated when MIXER_OVERFLOW flag is 0.

Referenced by XDfePrach_GetStatus().