| dp12rxss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xdprxss.c File Reference

## Functions
u32 | XDpRxSs_CfgInitialize (XDpRxSs *InstancePtr, XDpRxSs_Config *CfgPtr, UINTPTR EffectiveAddr)
| This function initializes the DisplayPort Receiver Subsystem core. More...
void | XDpRxSs_Reset (XDpRxSs *InstancePtr)
| This function resets the DisplayPort Receiver Subsystem including all sub-cores. More...
u32 | XDpRxSs_Start (XDpRxSs *InstancePtr)
| This function starts the DisplayPort Receiver Subsystem including all sub-cores. More...
u32 | XDpRxSs_SetLinkRate (XDpRxSs *InstancePtr, u8 LinkRate)
| This function sets the data rate to be used by the DisplayPort RX Subsystem core. More...
u32 | XDpRxSs_SetLaneCount (XDpRxSs *InstancePtr, u8 LaneCount)
| This function sets the number of lanes to be used by DisplayPort RX Subsystem core. More...
u32 | XDpRxSs_ExposePort (XDpRxSs *InstancePtr, u8 Port)
| This function allows the user to select number of ports to be exposed when replying to a LINK_ADDRESS sideband message and hides rest of the ports. More...
u32 | XDpRxSs_CheckLinkStatus (XDpRxSs *InstancePtr)
| This function checks if the receiver's DisplayPort Configuration Data (DPCD) indicates that the receiver has achieved clock recovery, channel equalization, symbol lock, and interlane alignment for all lanes currently in use. More...
void | XDpRxSs_SetUserPixelWidth (XDpRxSs *InstancePtr, u8 UserPixelWidth)
| This function configures the number of pixels output through the user data interface. More...
u32 | XDpRxSs_HandleDownReq (XDpRxSs *InstancePtr)
| This function handles incoming sideband messages. More...