| v_hdmitxss1 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XV_HdmiTxSs1_DynHdr_Config Struct Reference

Dynamic HDR configuration structure. More...

## Data Fields
u64 | Address
| Dynamic HDR packet buffer address. More...
u16 | PktType
| 16 bit Packet Type More...
u16 | PktLength
| 16 bit Packet Length More...
u8 | GOF
| GOF Value 0 or 1 only. More...
u8 | FAPA
| FAPA Location 0 or 1 only. More...

## Detailed Description

Dynamic HDR configuration structure.

This contains 1 - buffer address which contains the Dynamic HDR packet, 2 - the packet type and length, 3 - Graphics Overlay Flag value 4 - FAPA Location

## Field Documentation

u64 XV_HdmiTxSs1_DynHdr_Config::Address

Dynamic HDR packet buffer address.

Referenced by XV_HdmiTxSs1_DynHdr_Cfg().

u8 XV_HdmiTxSs1_DynHdr_Config::FAPA

FAPA Location 0 or 1 only.

Referenced by XV_HdmiTxSs1_DynHdr_Cfg().

u8 XV_HdmiTxSs1_DynHdr_Config::GOF

GOF Value 0 or 1 only.

Referenced by XV_HdmiTxSs1_DynHdr_Cfg().

u16 XV_HdmiTxSs1_DynHdr_Config::PktLength

16 bit Packet Length

Referenced by XV_HdmiTxSs1_DynHdr_Cfg().

u16 XV_HdmiTxSs1_DynHdr_Config::PktType

16 bit Packet Type

Referenced by XV_HdmiTxSs1_DynHdr_Cfg().