| cfupmc Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XCfupmc Struct Reference

The XCfupmc driver instance data structure. More...

## Data Fields
XCfupmc_Config | Config
| Hardware configuration. More...
u32 | IsReady
| Device and the driver instance are initialized. More...
u8 | DeCompress
| Indicates whether compression is is enabled or not. More...
u8 | Crc32Check
| Indicates if CRC32 is enabled or not. More...
u32 | Crc32Val
| Checksum value. More...
u8 | Crc8Dis
| Indicates if CRC8 is enabled or not. More...

## Detailed Description

The XCfupmc driver instance data structure.

A pointer to an instance data structure is passed around by functions to refer to a specific driver instance.

## Field Documentation

XCfupmc_Config XCfupmc::Config

Hardware configuration.

Referenced by XCfupmc_CfgInitialize().

u8 XCfupmc::Crc32Check

Indicates if CRC32 is enabled or not.

u32 XCfupmc::Crc32Val

Checksum value.

u8 XCfupmc::Crc8Dis

Indicates if CRC8 is enabled or not.

u8 XCfupmc::DeCompress

Indicates whether compression is is enabled or not.

u32 XCfupmc::IsReady

Device and the driver instance are initialized.

Referenced by XCfupmc_CfgInitialize().