| rtcpsu Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Examples

You can refer to the below stated example applications for more details on how to use rtcpsu driver.

# xrtcpsu_alarm_interrupt_example.c

Contains an example on how to use the XRtcpsu driver directly. This is the alarm example using the driver in interrupt mode.

For details, see xrtcpsu_alarm_interrupt_example.c.

# xrtcpsu_alarm_polled_example.c

Contains an example on how to use the XRtcpsu driver directly. This is the alarm example using the driver in polled mode.

For details, see xrtcpsu_alarm_polled_example.c.

# xrtcpsu_periodic_alarm_interrupt_example.c

Contains an example on how to use the XRtcpsu driver directly. This is the periodic alarm example using the driver in interrupt mode.

For details, see xrtcpsu_periodic_alarm_interrupt_example.c.

# xrtcpsu_seconds_interrupt_example.c

Contains an example on how to use the XRtcpsu driver directly. This is the seconds example using the driver in interrupt mode.

For details, see xrtcpsu_seconds_interrupt_example.c.

# xrtcpsu_seconds_polled_example.c

Contains an example on how to use the XRtcpsu driver directly. This is the seconds example using the driver in polled mode.

For details, see xrtcpsu_seconds_polled_example.c.

# xrtcpsu_set_calibration_example.c

Contains an example on how to use the XRtcpsu driver directly. This example contains the functions which updates the calibration register value.

For details, see xrtcpsu_set_calibration_example.c.

# xrtcpsu_set_time_example.c

Contains an example on how to use the XRtcpsu driver directly. This example contains the functions which updates the current time.

For details, see xrtcpsu_set_time_example.c.