| csi2tx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xcsi2tx_intr.c File Reference

## Functions
void | XCsi2Tx_IntrEnable (XCsi2Tx *InstancePtr, u32 Mask)
| This function will enable the interrupts present in the interrupt mask passed onto the function. More...
void | XCsi2Tx_IntrDisable (XCsi2Tx *InstancePtr, u32 Mask)
| This function will disable the interrupts present in the interrupt mask passed onto the function. More...
u32 | XCsi2Tx_GetIntrEnable (XCsi2Tx *InstancePtr)
| This function will get the interrupt mask set (enabled) in the CSI2 Tx core. More...
u32 | XCsi2Tx_GetIntrStatus (XCsi2Tx *InstancePtr)
| This function will get the list of interrupts pending in the Interrupt Status Register of the CSI2 Tx core. More...
void | XCsi2Tx_InterruptClear (XCsi2Tx *InstancePtr, u32 Mask)
| This function will clear the interrupts set in the Interrupt Status Register of the CSI2 Tx core. More...
int | XCsi2Tx_SetCallBack (XCsi2Tx *InstancePtr, u32 HandleType, void *Callbackfunc, void *Callbackref)
| This routine installs an asynchronous callback function for the given HandlerType: More...
void | XCsi2Tx_IntrHandler (void *InstancePtr)
| This function is the interrupt handler for the CSI2 Tx core. More...