| dfeequ Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeEqu_InterruptMask Struct Reference
Overview

Event status and interrupt mask. More...

## Data Fields
u32 | Mask [XDFEEQU_CHANNEL_NUM]
| [0,1] Mask status events. More...

## Detailed Description

Event status and interrupt mask.

## Field Documentation

u32 XDfeEqu_InterruptMask::Mask[XDFEEQU_CHANNEL_NUM]

[0,1] Mask status events.

Referenced by XDfeEqu_GetInterruptMask(), and XDfeEqu_SetInterruptMask().