| dsi Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xdsi.c File Reference

## Functions
u32 | XDsi_CfgInitialize (XDsi *InstancePtr, XDsi_Config *CfgPtr, UINTPTR EffectiveAddr)
| Initialize the XDsi instance provided by the caller based on the given Config structure. More...
void | XDsi_Reset (XDsi *InstancePtr)
| This function will do a reset of the IP. More...
u32 | XDsi_DefaultConfigure (XDsi *InstancePtr)
| This function will configure protocol reg with video mode, Blank packet mode, Blank packet Type, End of Transmisstion packet. More...
u32 | XDsi_Activate (XDsi *InstancePtr, XDsi_Selection Flag)
| This function will enable/disable the IP Core to start processing. More...
void | XDsi_SendShortPacket (XDsi *InstancePtr, XDsi_ShortPacket *ShortPacket)
| This function will send the short packet to DSI controller Generic Short Packet Register. More...
void | XDsi_SendLongPacket (XDsi *InstancePtr, XDsiTx_CmdModePkt *CmdPacket)
int | XDsi_SendCmdModePkt (XDsi *InstancePtr, XDsiTx_CmdModePkt *CmdPktData)
int | XDsi_SetMode (XDsi *InstancePtr, XDsi_DsiModeType mode)
void | XDsi_GetConfigParams (XDsi *InstancePtr, XDsi_ConfigParameters *ConfigInfo)
| This function will get the information from the GUI settings and other protocol control register values like video mode, Blank packet type, Packet Mode, EOTP value. More...
s32 | XDsi_SetVideoInterfaceTiming (XDsi *InstancePtr, XDsi_VideoMode VideoMode, XVidC_VideoMode Resolution, u16 BurstPacketSize)
| This function Set Timning mode and Resolution as per that it populate with Peripheral Timing Parameters from the video common library. More...
s32 | XDsi_SetCustomVideoInterfaceTiming (XDsi *InstancePtr, XDsi_VideoMode VideoMode, XDsi_VideoTiming *Timing)
| XDsi_SetCustomVideoInterfaceTiming Set Timning mode and Resolution as per user input. More...