| dphy Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xdphy_example_selftest.c File Reference

## Overview

    MODIFICATION HISTORY:

    Ver   Who       Date     Changes

    1.1   ms     01/23/17  Modified xil_printf statement in main function to
                           ensure that "Successfully ran" and "Failed" strings
                           are available in all examples. This is a fix for
                           CR-965028.
          ms     04/05/17  Modified Comment lines in functions to
                           recognize it as documentation block for doxygen
                           generation of examples.

## Functions
u32 | DphySelfTestExample (u32 DeviceId)
| This function checks if the HS_TIMEOUT from the generated file matches the value present in the corresponding configuration register. More...
int | main ()
| The entry point for this example. More...

## Function Documentation

u32 DphySelfTestExample | ( | u32 | DeviceId | ) |

This function checks if the HS_TIMEOUT from the generated file matches the value present in the corresponding configuration register.

Parameters

  DeviceId | is the DPHY device id.

Returns
  - XST_SUCCESS if values match

- XST_FAILURE if values differ.

Note
  None.

References XDphy_Config::BaseAddr, XDphy_CfgInitialize(), XDphy_GetRegIntfcPresent(), XDphy_LookupConfig(), and XDphy_SelfTest().

Referenced by main().

int main | ( |  | ) |

The entry point for this example.

It invokes the example function, and reports the execution status.

Parameters

  None. |

Returns
  - XST_SUCCESS if example finishes successfully
  - XST_FAILURE if example fails.

Note
  None.

References DphySelfTestExample().