| uartps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xuartps.c File Reference

## Functions
s32 | XUartPs_CfgInitialize (XUartPs *InstancePtr, XUartPs_Config *Config, u32 EffectiveAddr)
| Initializes a specific XUartPs instance such that it is ready to be used. More...
u32 | XUartPs_Send (XUartPs *InstancePtr, u8 *BufferPtr, u32 NumBytes)
| This functions sends the specified buffer using the device in either polled or interrupt driven mode. More...
u32 | XUartPs_Recv (XUartPs *InstancePtr, u8 *BufferPtr, u32 NumBytes)
| This function attempts to receive a specified number of bytes of data from the device and store it into the specified buffer. More...
s32 | XUartPs_SetBaudRate (XUartPs *InstancePtr, u32 BaudRate)
| Sets the baud rate for the device. More...