| aiengine Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

xsock_servtest.c File Reference

## Overview

This file contains the entry point for the server socket connection test.

    MODIFICATION HISTORY:

    Ver   Who     Date     Changes

    1.0  Naresh  02/19/2018  Initial creation
    1.1  Naresh  07/11/2018  Updated copyright info
    1.2  Nishad  12/05/2018  Renamed ME attributes to AIE

#define | XAIE_BUFLEN 50
| Buffer length for socket communication. More...
char | rcvmsgpass [] = "SERVER: Receive message successful"
| < Server socket receive data success message More...
int | main (int argc, char *argv[])
| This is the main entry point for the server socket test. More...

## Macro Definition Documentation

#define XAIE_BUFLEN 50

Buffer length for socket communication.

Referenced by main().

## Function Documentation

int main | ( | int | argc,
|  | char * | argv[]
| ) |  |

This is the main entry point for the server socket test.

Parameters

  argc | : Number of command line arguments.
  argv[0] | : File name.
  argv[1] | : Port number for the socket connection.

Returns
  0 on success, else 1.

Note
  None.

References XAIE_BUFLEN.

## Variable Documentation

char rcvmsgpass[] = "SERVER: Receive message successful"

< Server socket receive data success message

Server socket receive data fail message