| v_frmbuf_rd Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XV_frmbufrd Struct Reference

Driver instance data. More...

## Data Fields
XV_frmbufrd_Config | Config
| Hardware Configuration. More...
u32 | IsReady
| Device is initialized and ready. More...

## Detailed Description

Driver instance data.

An instance must be allocated for each core in use.

## Field Documentation

XV_frmbufrd_Config XV_frmbufrd::Config

Hardware Configuration.

Referenced by XVFrmbufRd_DbgReportStatus(), XVFrmbufRd_Get_FidErrorCount(), XVFrmbufRd_Get_FidErrorOut(), XVFrmbufRd_Get_FidOutMode(), XVFrmbufRd_Get_FieldOut(), XVFrmbufRd_GetFieldID(), XVFrmbufRd_Set_FidOutMode(), XVFrmbufRd_SetBufferAddr(), XVFrmbufRd_SetChromaBufferAddr(), XVFrmbufRd_SetFieldID(), XVFrmbufRd_SetMemFormat(), and XVFrmbufRd_SetVChromaBufferAddr().

u32 XV_frmbufrd::IsReady

Device is initialized and ready.

Referenced by XVFrmbufRd_InterruptHandler().