| uartps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XUartPs_Config Struct Reference
Overview

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
u32 | BaseAddress
| Base address of device (IPIF) More...
u32 | InputClockHz
| Input clock frequency. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

u32 XUartPs_Config::BaseAddress

Base address of device (IPIF)

Referenced by UartPsHelloWorldExample(), UartPsIntrExample(), UartPsPolledExample(), UartPsSelfTestExample(), XUartPs_CfgInitialize(), XUartPs_GetDataFormat(), XUartPs_GetFifoThreshold(), XUartPs_GetFlowDelay(), XUartPs_GetInterruptMask(), XUartPs_GetModemStatus(), XUartPs_GetOperMode(), XUartPs_GetOptions(), XUartPs_GetRecvTimeout(), XUartPs_InterruptHandler(), XUartPs_IsSending(), XUartPs_Recv(), XUartPs_SelfTest(), XUartPs_Send(), XUartPs_SetBaudRate(), XUartPs_SetDataFormat(), XUartPs_SetFifoThreshold(), XUartPs_SetFlowDelay(), XUartPs_SetInterruptMask(), XUartPs_SetOperMode(), XUartPs_SetOptions(), and XUartPs_SetRecvTimeout().

u16 XUartPs_Config::DeviceId

Unique ID of device.

u32 XUartPs_Config::InputClockHz

Input clock frequency.

Referenced by XUartPs_CfgInitialize(), and XUartPs_SetBaudRate().