| hdcp1x Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XHdcp1x_RxEncyptionWatch Struct Reference
Overview

This typedef is used to keep a tab on the changes in the encryption status of the HDCP receiver, depending on whether the incoming data non the receiver is HDCP protected or not. More...

## Data Fields
u8 | PreviousState
| Previous state of encryption. More...
u8 | CurrentState
| Current state of encryption. More...

## Detailed Description

This typedef is used to keep a tab on the changes in the encryption status of the HDCP receiver, depending on whether the incoming data non the receiver is HDCP protected or not.

## Field Documentation

u8 XHdcp1x_RxEncyptionWatch::CurrentState

Current state of encryption.

u8 XHdcp1x_RxEncyptionWatch::PreviousState

Previous state of encryption.