| spips Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XSpiPs_Config Struct Reference
Overview

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
u32 | BaseAddress
| Base address of the device. More...
u32 | InputClockHz
| Input clock frequency. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

u32 XSpiPs_Config::BaseAddress

Base address of the device.

Referenced by SpiPsEepromIntrExample(), SpiPsEepromPolledExample(), SpiPsFlashIntrExample(), SpiPsFlashPolledExample(), SpiPsSelfTestExample(), SpiPsSlavePolledExample(), SpiPsTpmPolledExample(), SpiSlaveRead(), SpiSlaveWrite(), XSpiPs_Abort(), XSpiPs_CfgInitialize(), XSpiPs_GetClkPrescaler(), XSpiPs_GetDelays(), XSpiPs_GetOptions(), XSpiPs_InterruptHandler(), XSpiPs_PolledTransfer(), XSpiPs_Reset(), XSpiPs_SelfTest(), XSpiPs_SetClkPrescaler(), XSpiPs_SetDelays(), XSpiPs_SetOptions(), XSpiPs_SetSlaveSelect(), and XSpiPs_Transfer().

u16 XSpiPs_Config::DeviceId

Unique ID of device.

Referenced by XSpiPs_CfgInitialize().

u32 XSpiPs_Config::InputClockHz

Input clock frequency.

Referenced by XSpiPs_CfgInitialize().