| v_deinterlacer Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XV_deinterlacer_Config Struct Reference

This typedef contains configuration information for the DEINT core. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | BaseAddress
| The base address of the core instance. More...
u16 | NumVidComponents
| Number of Video Components. More...
u16 | MaxDataWidth
| Maximum Data width of each channel. More...

## Detailed Description

This typedef contains configuration information for the DEINT core.

Each core instance should have a configuration structure associated.

## Field Documentation

UINTPTR XV_deinterlacer_Config::BaseAddress

The base address of the core instance.

Referenced by XV_DeintDbgReportStatus().

u16 XV_deinterlacer_Config::DeviceId

Unique ID of device.

u16 XV_deinterlacer_Config::MaxDataWidth

Maximum Data width of each channel.

u16 XV_deinterlacer_Config::NumVidComponents

Number of Video Components.