| v_sditx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XV_SdiTx_Config Struct Reference

This typedef contains configuration information for the SDI TX core. More...

## Data Fields
u16 | DeviceId
| DeviceId is the unique ID of the SDI TX core. More...
UINTPTR | BaseAddress
| BaseAddress is the physical base address of the core's registers. More...
u8 | InsertCSTRST352
| Insert ST352 in C stream. More...

## Detailed Description

This typedef contains configuration information for the SDI TX core.

Each SDI TX device should have a configuration structure associated.

## Field Documentation

UINTPTR XV_SdiTx_Config::BaseAddress

BaseAddress is the physical base address of the core's registers.

Referenced by XV_SdiTx_Axi4sBridgeVtcDisable(), XV_SdiTx_Axi4sBridgeVtcEnable(), XV_SdiTx_CfgInitialize(), XV_SdiTx_ClearDetectedError(), XV_SdiTx_ClearYCbCr444_RGB_10bit(), XV_SdiTx_DebugInfo(), XV_SdiTx_GetIntrEnable(), XV_SdiTx_GetIntrStatus(), XV_SdiTx_InterruptClear(), XV_SdiTx_IntrDisable(), XV_SdiTx_IntrEnable(), XV_SdiTx_IntrHandler(), XV_SdiTx_ReportDetectedError(), XV_SdiTx_SelfTest(), XV_SdiTx_SetColorFormat(), XV_SdiTx_SetCoreSettings(), XV_SdiTx_SetPayloadLineNum(), XV_SdiTx_SetVidBridgeMode(), XV_SdiTx_SetYCbCr444_RGB_10bit(), XV_SdiTx_ST352CStreamEnable(), XV_SdiTx_ST352CSwitch3GA(), XV_SdiTx_StartSdi(), XV_SdiTx_StopSdi(), XV_SdiTx_StreamStart(), XV_SdiTx_VidBridgeDisable(), XV_SdiTx_VidBridgeEnable(), and XV_SdiTxSelfTestExample().

u16 XV_SdiTx_Config::DeviceId

DeviceId is the unique ID of the SDI TX core.

u8 XV_SdiTx_Config::InsertCSTRST352

Insert ST352 in C stream.