| sdps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xsdps_raw_example.c File Reference

## Overview

This example is used to test read and write transfers on SD/eMMC interface.

Please note that running this example will modify the card contents and file system information will be erased in the card. Card will need to be re-formatted.

Modify the offset and Size macros to test different SD memory offset and size.

     MODIFICATION HISTORY:

     Ver    Who     Date     Changes

     3.9    mn  12/02/19 First release
     3.10   mn  09/17/20 Fix sector offset issue with Non-HCS SD cards
     4.2   ro     06/12/23 Added support for system device-tree flow.

## Functions
int | main (void)
| Main function to call the SD example. More...

## Function Documentation

int main | ( | void |  | ) |

Main function to call the SD example.

Returns
  XST_SUCCESS if successful, otherwise XST_FAILURE.

Note
  None