| tmr_manager Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Typedefs | Functions
xtmr_manager_intr.c File Reference

## Typedefs
typedef void(* | Handler )(XTMR_Manager *InstancePtr)
| This function is the handler which performs processing to send data to the TMR_Manager. More...

## Functions
void | XTMR_Manager_SetHandler (XTMR_Manager *InstancePtr, XTMR_Manager_Handler FuncPtr, void *CallBackRef)
| This function sets the handler that will be called when an event (interrupt) occurs in the driver. More...
void | XTMR_Manager_InterruptHandler (XTMR_Manager *InstancePtr)
| This function is the interrupt handler for the TMR Manager driver. More...
void | XTMR_Manager_DisableInterrupt (XTMR_Manager *InstancePtr)
| This function disables the core interrupt. More...
void | XTMR_Manager_EnableInterrupt (XTMR_Manager *InstancePtr, u32 Mask)
| This function enables the core interrupt such that an interrupt will occur when any of the SEM status signals indicated by the mask are changed. More...