| tmr_inject Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XTMR_Inject_Config Struct Reference
Overview

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | RegBaseAddr
| Register base address. More...
u8 | MagicByte
| Magic Byte parameter. More...
u8 | CpuId
| CPU to Inject parameter. More...
u8 | LMBAddrWidth
| LMB address width. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

u8 XTMR_Inject_Config::CpuId

CPU to Inject parameter.

u16 XTMR_Inject_Config::DeviceId

Unique ID of device.

u8 XTMR_Inject_Config::LMBAddrWidth

LMB address width.

Referenced by XTMR_Inject_CfgInitialize().

u8 XTMR_Inject_Config::MagicByte

Magic Byte parameter.

Referenced by XTMR_Inject_CfgInitialize().

UINTPTR XTMR_Inject_Config::RegBaseAddr

Register base address.

Referenced by XTMR_Inject_Initialize().