| dp12 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDp_TxSinkConfig Struct Reference
Overview

This typedef contains configuration information about the RX device. More...

## Data Fields
u8 | DpcdRxCapsField [16]
| The first 16 bytes of the raw capabilities field of the RX device's DisplayPort Configuration Data (DPCD). More...
u8 | LaneStatusAdjReqs [6]
| This is a raw read of the RX device's status registers. More...

## Detailed Description

This typedef contains configuration information about the RX device.

## Field Documentation

u8 XDp_TxSinkConfig::DpcdRxCapsField[16]

The first 16 bytes of the raw capabilities field of the RX device's DisplayPort Configuration Data (DPCD).

u8 XDp_TxSinkConfig::LaneStatusAdjReqs[6]

This is a raw read of the RX device's status registers.

The first 4 bytes correspond to the lane status associated with clock recovery, channel equalization, symbol lock, and interlane alignment. The remaining 2 bytes represent the pre-emphasis and voltage swing level adjustments requested by the RX device.