| sysmonpsu Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions | Variables
xsysmonpsu_sinit.c File Reference

## Functions
XSysMonPsu_Config * | XSysMonPsu_LookupConfig (u16 DeviceId)
| This function looks for the device configuration based on the unique device ID. More...

## Variables
XSysMonPsu_Config | XSysMonPsu_ConfigTable [XPAR_XSYSMONPSU_NUM_INSTANCES]
| This table contains configuration information for SYSMON device in the system. More...

## Function Documentation

XSysMonPsu_Config* XSysMonPsu_LookupConfig | ( | u16 | DeviceId | ) |

This function looks for the device configuration based on the unique device ID.

The table XSysmonPsu_ConfigTable[] contains the configuration information for each device in the system.

Parameters

  DeviceId | is the unique device ID of the device being looked up.

Returns
  A pointer to the configuration table entry corresponding to the given device ID, or NULL if no match is found.

Note
  None.

Referenced by SysMonPsuAMSExample(), SysMonPsuIntrExample(), SysMonPsuPolledPrintfExample(), and SysMonPsuSingleChannelIntrExample().

## Variable Documentation

XSysMonPsu_Config XSysMonPsu_ConfigTable[XPAR_XSYSMONPSU_NUM_INSTANCES]

This table contains configuration information for SYSMON device in the system.