| axiethernet Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XAvb_RtcFormat Struct Reference

This typedef defines the format for the Real Time Clock (RTC). More...

## Data Fields
u16 | SecondsUpper
| Upper 16-bits of seconds field. More...
u32 | SecondsLower
| Lower 32-bits of seconds field. More...
u32 | NanoSeconds
| 32-bit nanoseconds field More...

## Detailed Description

This typedef defines the format for the Real Time Clock (RTC).

The RTC contains a 48-bit seconds field (split into upper and lower sections) and a 32-bit nano-seconds field.

## Field Documentation

u32 XAvb_RtcFormat::NanoSeconds

32-bit nanoseconds field

Referenced by XAvb_CalcRtcOffset(), XAvb_ReadRtc(), XAvb_SendPDelayRespFollowUp(), and XAvb_WriteRtcOffset().

u32 XAvb_RtcFormat::SecondsLower

Lower 32-bits of seconds field.

Referenced by XAvb_CalcRtcOffset(), XAvb_ReadRtc(), XAvb_SendPDelayRespFollowUp(), and XAvb_WriteRtcOffset().

u16 XAvb_RtcFormat::SecondsUpper

Upper 16-bits of seconds field.

Referenced by XAvb_CalcRtcOffset(), XAvb_ReadRtc(), XAvb_SendPDelayRespFollowUp(), and XAvb_WriteRtcOffset().