| spdif Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XSpdif_Config Struct Reference
Overview

This typedef contains configuration information for the XSpdif. More...

## Data Fields
u32 | DeviceId
| DeviceId is the unique ID of XSpdif. More...
UINTPTR | BaseAddress
| BaseAddress of the XSpdif Transmitter or Receiver. More...

## Detailed Description

This typedef contains configuration information for the XSpdif.

## Field Documentation

UINTPTR XSpdif_Config::BaseAddress

BaseAddress of the XSpdif Transmitter or Receiver.

Referenced by SpdifSelfTestExample(), XSpdif_CfgInitialize(), XSpdif_Enable(), XSpdif_GetFs(), XSpdif_Initialize(), XSpdif_IntrHandler(), XSpdif_ResetFifo(), XSpdif_Rx_GetChA_UserData(), XSpdif_Rx_GetChB_UserData(), XSpdif_Rx_GetChStat(), XSpdif_SetClkConfig(), and XSpdif_SoftReset().

u32 XSpdif_Config::DeviceId

DeviceId is the unique ID of XSpdif.