| nandpsu Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xnandpsu_bbm.c File Reference

## Functions
void | XNandPsu_InitBbtDesc (XNandPsu *InstancePtr)
| This function initializes the Bad Block Table(BBT) descriptors with a predefined pattern for searching Bad Block Table(BBT) in flash. More...
s32 | XNandPsu_ScanBbt (XNandPsu *InstancePtr)
| This function reads the Bad Block Table(BBT) if present in flash. More...
s32 | XNandPsu_IsBlockBad (XNandPsu *InstancePtr, u32 Block)
| This function checks whether a block is bad or not. More...
s32 | XNandPsu_MarkBlockBad (XNandPsu *InstancePtr, u32 Block)
| This function marks a block as bad in the RAM based Bad Block Table(BBT). More...