| tmr_manager Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xtmr_manager_low_level_example.c File Reference

## Overview

This file contains a design example using the low-level driver functions and macros of the TMR_Manager driver (XTMR_Manager).

Note

The user must provide a physical loopback such that data which is transmitted will be received.

MODIFICATION HISTORY:

    Ver   Who  Date  Changes

    1.0   sa   04/05/17 First release
    1.7   adk  04/04/25 Ported example to the SDT flow.

## Functions
int | TMR_ManagerLowLevelExample (u32 TMR_ManagerBaseAddress)
| This function does a minimal test on the TMR_Manager device using low-level driver macros and functions. More...
int | main (void)
| Main function to call the example. More...

## Function Documentation

int main | ( | void |  | ) |

Main function to call the example.

Parameters

  None. |

Returns
  XST_SUCCESS if successful, XST_FAILURE if unsuccessful.

Note
  None.

References TMR_ManagerLowLevelExample().

int TMR_ManagerLowLevelExample | ( | u32 | TMR_ManagerBaseAddress | ) |

This function does a minimal test on the TMR_Manager device using low-level driver macros and functions.

Parameters

  TMR_ManagerBaseAddress | is the base address of the TMR_Manager device and is the XPAR_<TMRMANAGER_instance>_BASEADDR value from xparameters.h.

Returns
  XST_SUCCESS if successful, XST_FAILURE if unsuccessful.

Note
  None.

Referenced by main().