| axis_switch Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Data Structures | Macros | Functions
xaxis_switch.h File Reference

## Data Structures
struct | XAxis_Switch_Config
| This typedef contains configuration information for the AXI4-Stream Switch core. More...
struct | XAxis_Switch
| The AXI4-Stream Switch driver instance data. More...

## Macros
#define | XAXIS_SWITCH_H_
| Prevent circular inclusions by using protection macros. More...
#define | XAxisScr_RegUpdateEnable(InstancePtr)
| This macro enables register updates. More...
#define | XAxisScr_RegUpdateDisable(InstancePtr)
| This macro disables register updates. More...

## Functions
XAxis_Switch_Config * | XAxisScr_LookupConfig (u16 DeviceId)
| This function returns a reference to an XAxis_Switch_Config structure based on the core id, DeviceId. More...
s32 | XAxisScr_CfgInitialize (XAxis_Switch *InstancePtr, XAxis_Switch_Config *CfgPtr, UINTPTR EffectiveAddr)
| This function initializes the AXI4-Stream Switch core. More...
void | XAxisScr_MiPortEnable (XAxis_Switch *InstancePtr, u8 MiIndex, u8 SiIndex)
| This function enables the MUX port specified by a MI index and links with desired SI, indicated by a SiIndex. More...
void | XAxisScr_MiPortDisable (XAxis_Switch *InstancePtr, u8 MiIndex)
| This function disables the MUX port specified by a MI index and un-link SI, set previously. More...
s32 | XAxisScr_IsMiPortEnabled (XAxis_Switch *InstancePtr, u8 MiIndex, u8 SiIndex)
| This function returns the status of whether MUX is sourced from desired SI. More...
s32 | XAxisScr_IsMiPortDisabled (XAxis_Switch *InstancePtr, u8 MiIndex)
| This function returns the status of whether MUX is disabled. More...
void | XAxisScr_MiPortDisableAll (XAxis_Switch *InstancePtr)
| This function disables all the MUX port, in turn removes association with desired SI. More...
s32 | XAxisScr_SelfTest (XAxis_Switch *InstancePtr)
| This function performs self test on AXI4-Stream Switch core registers. More...