| dfemix Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeMix_TriggerCfg Struct Reference
Overview

All IP triggers. More...

## Data Fields
XDfeMix_Trigger | Activate
                       Switch between "Initialized",
ultra-low power state, and "Operational". More...
XDfeMix_Trigger | LowPower
                       Switch between "Low-power"
and "Operational" state. More...
XDfeMix_Trigger | CCUpdate
                       Transition to next CC
configuration. More...
XDfeMix_Trigger | Switch
                     Switch between Downlink and Uplink datapth
configuration. More...

## Detailed Description

All IP triggers.

## Field Documentation

XDfeMix_Trigger XDfeMix_TriggerCfg::Activate

                       Switch between "Initialized",

ultra-low power state, and "Operational".

One-shot trigger, disabled following a single event.

Referenced by XDfeMix_AddCCExample(), XDfeMix_GetTriggersCfg(), XDfeMix_MultiAddCCExample(), and XDfeMix_SetTriggersCfg().

XDfeMix_Trigger XDfeMix_TriggerCfg::CCUpdate

                       Transition to next CC

configuration.

Will initiate flush based on CC configuration.

Referenced by XDfeMix_AddCCExample(), XDfeMix_GetTriggersCfg(), XDfeMix_MultiAddCCExample(), and XDfeMix_SetTriggersCfg().

XDfeMix_Trigger XDfeMix_TriggerCfg::LowPower

                       Switch between "Low-power"

and "Operational" state.

Referenced by XDfeMix_GetTriggersCfg(), and XDfeMix_SetTriggersCfg().

XDfeMix_Trigger XDfeMix_TriggerCfg::Switch

                     Switch between Downlink and Uplink datapth

configuration.

Will initiate flush based on CC configuration.

Referenced by XDfeMix_GetTriggersCfg(), and XDfeMix_SetTriggersCfg().