| usbpsu Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xusbpsu_ep0handler.c File Reference

## Functions
s32 | XUsbPsu_RecvSetup (struct XUsbPsu *InstancePtr)
| Initiates DMA on control endpoint 0 to receive setup packet. More...
void | XUsbPsu_Ep0XferComplete (struct XUsbPsu *InstancePtr, const struct XUsbPsu_Event_Epevt *Event)
| Handles transfer complete event of control endpoints EP0 OUT and EP0 IN. More...
void | XUsbPsu_Ep0XferNotReady (struct XUsbPsu *InstancePtr, const struct XUsbPsu_Event_Epevt *Event)
| Handles transfer not ready event of control endpoints EP0 OUT and EP0 IN. More...
s32 | XUsbPsu_Ep0Send (struct XUsbPsu *InstancePtr, u8 *BufferPtr, u32 BufferLen)
| Initiates DMA to send data on control endpoint EP0 IN to host. More...
s32 | XUsbPsu_Ep0Recv (struct XUsbPsu *InstancePtr, u8 *BufferPtr, u32 Length)
| Initiates DMA to receive data on control endpoint EP0 OUT from host. More...