| usbps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xusbps_intr_example.c File Reference

## Overview

This file contains an example of how to use the USB driver with the USB controller in DEVICE mode.

      MODIFICATION HISTORY:

      Ver   Who     Date     Changes

      1.00a wgr/nm  10/09/10 First release
      1.01a nm      03/05/10 Included xpseudo_asm.h instead of xpseudo_asm_gcc.h
      1.04a nm      02/05/13 Fixed CR# 696550.
                             Added template code for Vendor request.
      1.06a kpc             11/11/13 Fixed CR#759458, cacheInvalidate size should be
                                     ailgned to cache line size.
      2.1   kpc    04/28/14 Cleanup and removed unused functions
      2.4   vak    04/01/19 Fixed IAR data_alignment warnings
      2.8   pm     07/07/23 Added support for system device-tree flow
    *

## Functions
int | main (void)
| Main function to call the USB interrupt example. More...

## Function Documentation

int main | ( | void |  | ) |

Main function to call the USB interrupt example.

Parameters

  None |

Returns
  - XST_SUCCESS if successful
  - XST_FAILURE on error