| axiethernet Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XAvb_SignallingFrameData Struct Reference

The Signalling frame defines the delays to be used between Sync Frames, Link Delay measurements and Announce Frame events. More...

## Data Fields
u16 | SyncIntervalDuration
| Sync Interval in units of 1/128 seconds. More...
u16 | LinkDelayIntervalDuration
| Link Delay Interval in units of 1/128 seconds. More...
u16 | AnnounceIntervalDuration
| Announce Interval in units of 1/128 seconds. More...

## Detailed Description

The Signalling frame defines the delays to be used between Sync Frames, Link Delay measurements and Announce Frame events.

## Field Documentation

u16 XAvb_SignallingFrameData::AnnounceIntervalDuration

Announce Interval in units of 1/128 seconds.

Referenced by XAvb_DecodeRxSignaling(), XAvb_PtpTimerInterruptHandler(), and XAvb_Reset().

u16 XAvb_SignallingFrameData::LinkDelayIntervalDuration

Link Delay Interval in units of 1/128 seconds.

Referenced by XAvb_DecodeRxSignaling(), XAvb_PtpTimerInterruptHandler(), and XAvb_Reset().

u16 XAvb_SignallingFrameData::SyncIntervalDuration

Sync Interval in units of 1/128 seconds.

Referenced by XAvb_DecodeRxSignaling(), XAvb_PtpTimerInterruptHandler(), and XAvb_Reset().