| dphy Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDphy Struct Reference
Overview

The XDphy Controller driver instance data. More...

## Data Fields
XDphy_Config | Config
| Hardware Configuration. More...
u32 | IsReady
| Driver is ready. More...

## Detailed Description

The XDphy Controller driver instance data.

The user is required to allocate a variable of this type for every XDphy device in the system. A pointer to a variable of this type is then passed to the driver API functions.

## Field Documentation

XDphy_Config XDphy::Config

Hardware Configuration.

Referenced by XDphy_Activate(), XDphy_CfgInitialize(), XDphy_ClearDataLane(), XDphy_Configure(), XDphy_GetClkLaneMode(), XDphy_GetClkLaneStatus(), XDphy_GetDataLaneMode(), XDphy_GetDataLaneStatus(), XDphy_GetDLCalibStatus(), XDphy_GetInfo(), XDphy_GetPacketCount(), XDphy_GetRegIntfcPresent(), XDphy_Reset(), and XDphy_SelfTest().

u32 XDphy::IsReady

Driver is ready.

Referenced by XDphy_CfgInitialize(), and XDphy_Reset().