| i3c Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xi3c.c File Reference

## Functions
void | XI3c_ConfigIbi (XI3c *InstancePtr, u8 DevCount)
| This configure target address and BCR register values of available devices to the controller RAM. More...
void | XI3C_BusInit (XI3c *InstancePtr)
| Initializes the XI3c slaves devices by disable/enable events and reset dynamic addresses. More...
s32 | XI3c_CfgInitialize (XI3c *InstancePtr, XI3c_Config *ConfigPtr, u32 EffectiveAddr)
| Initializes a specific XI3c instance such that the driver is ready to use. More...
void | XI3c_FillCmdFifo (XI3c *InstancePtr, XI3c_Cmd *Cmd)
| Fill I3C Command fifo. More...
void | XI3c_WriteTxFifo (XI3c *InstancePtr)
| Fill I3C Write Tx FIFO. More...
void | XI3c_ReadRxFifo (XI3c *InstancePtr)
| Read RX I3C FIFO. More...
s32 | XI3c_DynaAddrAssign (XI3c *InstancePtr, u8 DynaAddr[], u8 DevCount)
| This function sends dynamic Address Assignment for available devices. More...