| dfemix Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xdfemix_one_instance_initialization_example.c File Reference

## Overview

This file contains a load coefficients example.

    MODIFICATION HISTORY:

    Ver   Who    Date     Changes

    1.1   dc     07/21/21 Add and reorganise examples
    1.5   dc     10/24/22 Switching Uplink/Downlink support

## Functions
int | XDfeMix_SelfTestExample ()
| This function runs the DFE Mixer device using the driver APIs. More...

## Function Documentation

int XDfeMix_SelfTestExample | ( |  | ) |

This function runs the DFE Mixer device using the driver APIs.

This function does the following tasks:

- Create and system initialize the device driver instance.
- Read SW and HW version numbers.
- Reset the device.
- Configure the device.
- Initialize the device.
- Activate the device.
- DeActivate the device.

Returns
  - XST_SUCCESS if the example has completed successfully.
  - XST_FAILURE if the example has failed.

References XDfeMix_Version::Major, XDfeMix_Version::Minor, XDfeMix_Version::Patch, XDfeMix_Version::Revision, XDfeMix_Init::TuserSelect, XDfeMix_Activate(), XDfeMix_Configure(), XDfeMix_Deactivate(), XDfeMix_GetVersions(), XDfeMix_Initialize(), XDfeMix_InstanceClose(), XDfeMix_InstanceInit(), XDfeMix_Reset(), XST_FAILURE, and XST_SUCCESS.

Referenced by main().