| dfeprach Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfePrach_DecimatorStatusOverrun Struct Reference
Overview

PRACH decimator overrun status. More...

## Data Fields
u32 | DecimatorOverrun
                   [0-1] Source of first occurrence of overflow
as signalled in ISR. More...
u32 | FirstAntennaOverruning
                         [0-7] Lowest number antenna on which
first overrun occurred. More...
u32 | FirstRCIdOverruning
                      [0-15] Lowest numbered Physical RACH
channel on which first overrun occurred. More...

## Detailed Description

PRACH decimator overrun status.

## Field Documentation

u32 XDfePrach_DecimatorStatusOverrun::DecimatorOverrun

                   [0-1] Source of first occurrence of overflow

as signalled in ISR.

That is, register only updated when DECIMATOR_OVERRUN flag is 0.

Referenced by XDfePrach_GetStatus().

u32 XDfePrach_DecimatorStatusOverrun::FirstAntennaOverruning

                         [0-7] Lowest number antenna on which

first overrun occurred.

Referenced by XDfePrach_GetStatus().

u32 XDfePrach_DecimatorStatusOverrun::FirstRCIdOverruning

                      [0-15] Lowest numbered Physical RACH

channel on which first overrun occurred.

Referenced by XDfePrach_GetStatus().