| sdps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- All
- Functions
- Variables
- Macros

- a
- c
- e
- h
- m
- s
- u
- w
- x

### - a -

- ADDRESS_BEYOND_32BIT : xsdps.h

### - c -

- CSD_SPEC_VER_3 : xsdps.h

### - e -

- ENABLE_HS400_MODE : xsdps.h
- EXT_CSD_DEVICE_TYPE_BYTE : xsdps.h
- EXT_CSD_DEVICE_TYPE_DDR_1V2_HIGH_SPEED : xsdps.h
- EXT_CSD_DEVICE_TYPE_DDR_1V2_HS400 : xsdps.h
- EXT_CSD_DEVICE_TYPE_DDR_1V8_HIGH_SPEED : xsdps.h
- EXT_CSD_DEVICE_TYPE_DDR_1V8_HS400 : xsdps.h
- EXT_CSD_DEVICE_TYPE_HIGH_SPEED : xsdps.h
- EXT_CSD_DEVICE_TYPE_SDR_1V2_HS200 : xsdps.h
- EXT_CSD_DEVICE_TYPE_SDR_1V8_HS200 : xsdps.h
- EXT_CSD_SEC_COUNT_BYTE1 : xsdps.h
- EXT_CSD_SEC_COUNT_BYTE2 : xsdps.h
- EXT_CSD_SEC_COUNT_BYTE3 : xsdps.h
- EXT_CSD_SEC_COUNT_BYTE4 : xsdps.h

### - h -

- HIGH_SPEED_SUPPORT : xsdps.h

### - m -

- MAX_TIMEOUT : xsdps.h
- MAX_TUNING_COUNT : xsdps.h

### - s -

- SCR_SPEC_VER_3 : xsdps.h
- SD_CLK_19_MHZ : xsdps.h
- SD_CLK_25_MHZ : xsdps.h
- SD_CLK_26_MHZ : xsdps.h
- SD_HS_MODE_ENABLE : xsdps.h

### - u -

- UHS_DDR50_SUPPORT : xsdps.h
- UHS_SDR104_SUPPORT : xsdps.h
- UHS_SDR12_SUPPORT : xsdps.h
- UHS_SDR25_SUPPORT : xsdps.h
- UHS_SDR50_SUPPORT : xsdps.h

### - w -

- WIDTH_4_BIT_SUPPORT : xsdps.h

### - x -

- XSDPS_ACMD41_3V3 : xsdps.h
- XSDPS_ACMD41_HCS : xsdps.h
- XSDPS_BLK_SIZE_512_MASK : xsdps.h
- XSDPS_CMD1_DUAL_VOL : xsdps.h
- XSDPS_CMD1_HIGH_VOL : xsdps.h
- XSDPS_CMD8_VOL_PATTERN : xsdps.h
- XSDPS_CT_ERROR : xsdps.h
- XSDPS_RESPOCR_READY : xsdps.h
- XSDPS_VERSAL_SD0_BASE : xsdps.h
- XSDPS_VERSAL_SD1_BASE : xsdps.h
- XSDPS_ZYNQMP_SD0_BASE : xsdps.h
- XSDPS_ZYNQMP_SD1_BASE : xsdps.h