| sd_fec Vitis Drivers API Documentation

- Overview
- Data Structures

- Data Structures
- Data Fields

Data Fields
XSdFecInterruptClass Struct Reference

Interrupt class. More...

## Data Fields
u8 | Intf
| Triggered due to interface or control error (ISR) More...
u8 | ECCSBit
| Triggered due to single-bit ECC error (ECC_ISR) More...
u8 | ECCMBit
| Triggered due to multi-bit ECC error (ECC_ISR) More...
u8 | RstReq
| Device requires reset. More...
u8 | ReprogReq
| Device requires reprogrammed. More...
u8 | ReCfgReq
| FPGA requires reprogrammed. More...

## Detailed Description

Interrupt class.

Members define interrupt class and action required

## Field Documentation

u8 XSdFecInterruptClass::ECCMBit

Triggered due to multi-bit ECC error (ECC_ISR)

u8 XSdFecInterruptClass::ECCSBit

Triggered due to single-bit ECC error (ECC_ISR)

u8 XSdFecInterruptClass::Intf

Triggered due to interface or control error (ISR)

u8 XSdFecInterruptClass::ReCfgReq

FPGA requires reprogrammed.

u8 XSdFecInterruptClass::ReprogReq

Device requires reprogrammed.

u8 XSdFecInterruptClass::RstReq

Device requires reset.