| axivdma Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XAxiVdma_FrameCounter Struct Reference
Overview

The XAxiVdmaFrameCounter structure contains the interrupt threshold settings for both the transmit and the receive channel. More...

## Data Fields
u8 | ReadFrameCount
| Interrupt threshold for Receive. More...
u8 | ReadDelayTimerCount
| Delay timer threshold for receive. More...
u8 | WriteFrameCount
| Interrupt threshold for transmit. More...
u8 | WriteDelayTimerCount
| Delay timer threshold for transmit. More...

## Detailed Description

The XAxiVdmaFrameCounter structure contains the interrupt threshold settings for both the transmit and the receive channel.