| rfdc Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xrfdc_gen3_clocked_example.c File Reference

## Overview

This file contains an example for Gen 3 using the rfdc hardware and RFSoC Data Converter driver.

This example does some writes to the hardware to do some sanity checks and does a reset to restore the original settings.

Users are expected to have a programmed CLK-104 module if using this example for ZCU208/216.

    MODIFICATION HISTORY:

    Ver   Who    Date     Changes

    8.1   cog    06/29/20 First release.
          cog    07/03/20 The metal_phys parameter is baremetal only.
          cog    07/03/20 Formatting and text changes.
    11.0  cog    07/12/21 Simplified clock distribution user interface.

## Functions
int | main (void)
| Main function that invokes the polled example in this file. More...

## Function Documentation

int main | ( | void |  | ) |

Main function that invokes the polled example in this file.

Parameters

  None. |

Returns
  - XRFDC_SUCCESS if the example has completed successfully.
  - XRFDC_FAILURE if the example has failed.

Note
  None.