| v_csc Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XV_csc_Config Struct Reference

This typedef contains configuration information for the CSC core. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | BaseAddress
| The base address of the core instance. More...
u16 | PixPerClk
| Samples Per Clock supported by core instance. More...
u16 | MaxWidth
| Maximum columns supported by core instance. More...
u16 | MaxHeight
| Maximum rows supported by core instance. More...
u16 | MaxDataWidth
| Maximum Data width of each channel. More...
u16 | Is422Enabled
| 4:2:2 color format supported by core instance More...
u16 | Is420Enabled
| 4:2:0 color format supported by core instance More...
u16 | IsDemoWindowEnabled
| CSC demo window supported by core instance. More...

## Detailed Description

This typedef contains configuration information for the CSC core.

Each core instance should have a configuration structure associated.

## Field Documentation

UINTPTR XV_csc_Config::BaseAddress

The base address of the core instance.

Referenced by XV_CscDbgReportStatus().

u16 XV_csc_Config::DeviceId

Unique ID of device.

u16 XV_csc_Config::Is420Enabled

4:2:0 color format supported by core instance

u16 XV_csc_Config::Is422Enabled

4:2:2 color format supported by core instance

u16 XV_csc_Config::IsDemoWindowEnabled

CSC demo window supported by core instance.

u16 XV_csc_Config::MaxDataWidth

Maximum Data width of each channel.

u16 XV_csc_Config::MaxHeight

Maximum rows supported by core instance.

u16 XV_csc_Config::MaxWidth

Maximum columns supported by core instance.

u16 XV_csc_Config::PixPerClk

Samples Per Clock supported by core instance.