| uartlite Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions | Variables
xuartlite_i.h File Reference

## Functions
unsigned int | XUartLite_SendBuffer (XUartLite *InstancePtr)
| This function sends a buffer that has been previously specified by setting up the instance variables of the instance. More...
unsigned int | XUartLite_ReceiveBuffer (XUartLite *InstancePtr)
| This function receives a buffer that has been previously specified by setting up the instance variables of the instance. More...
u8 | XUartLite_GetSR (XUartLite *InstancePtr)
| This function reads the status register and updates the error stats, before returning the status register value. More...

## Variables
XUartLite_Config | XUartLite_ConfigTable []
| The configuration table for UART Lite devices. More...