| i3c Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xi3c_master.c File Reference

## Functions
s32 | XI3c_SendTransferCmd (XI3c *InstancePtr, XI3c_Cmd *Cmd, u8 Data)
| This function sends the command. More...
s32 | XI3c_MasterSend (XI3c *InstancePtr, XI3c_Cmd *Cmd, u8 *MsgPtr, u16 ByteCount)
| This function initiates a interrupt mode send in master mode. More...
s32 | XI3c_MasterRecv (XI3c *InstancePtr, XI3c_Cmd *Cmd, u8 *MsgPtr, u16 ByteCount)
| This function initiates a interrupt mode receive in master mode. More...
s32 | XI3c_MasterSendPolled (XI3c *InstancePtr, XI3c_Cmd *Cmd, u8 *MsgPtr, u16 ByteCount)
| This function initiates a polled mode send in master mode. More...
s32 | XI3c_MasterRecvPolled (XI3c *InstancePtr, XI3c_Cmd *Cmd, u8 *MsgPtr, u16 ByteCount)
| This function initiates a polled mode receive in master mode. More...
void | XI3c_SetStatusHandler (XI3c *InstancePtr, XI3c_IntrHandler FunctionPtr)
| This function sets the status handler, which the driver calls when it encounters conditions that should be reported to the higher layer software. More...
void | XI3c_MasterInterruptHandler (XI3c *InstancePtr)
| The interrupt handler for the master mode. More...
s32 | XI3c_IbiRecv (XI3c *InstancePtr, u8 *MsgPtr)
| This function setup for receive during IBI in interrupt mode. More...
s32 | XI3c_IbiRecvPolled (XI3c *InstancePtr, u8 *MsgPtr)
| This function receives data during IBI in polled mode. More...