| rtcpsu Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XRtcPsu_Config Struct Reference
Overview

This typedef contains configuration information for a device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | BaseAddr
| Register base address. More...

## Detailed Description

This typedef contains configuration information for a device.

## Field Documentation

UINTPTR XRtcPsu_Config::BaseAddr

Register base address.

Referenced by RtcPsuAlarmIntrExample(), RtcPsuAlarmPolledExample(), RtcPsuPeriodicAlarmIntrExample(), RtcPsuSecondsIntrExample(), RtcPsuSecondsPolledExample(), RtcPsuSetCalibrationExample(), RtcPsuSetTimeExample(), XRtcPsu_CfgInitialize(), XRtcPsu_ClearInterruptMask(), XRtcPsu_GetCurrentTime(), XRtcPsu_InterruptHandler(), XRtcPsu_IsAlarmEventGenerated(), XRtcPsu_IsSecondsEventGenerated(), XRtcPsu_SelfTest(), XRtcPsu_SetAlarm(), XRtcPsu_SetInterruptMask(), and XRtcPsu_SetTime().

u16 XRtcPsu_Config::DeviceId

Unique ID of device.

Referenced by XRtcPsu_CfgInitialize().