| mipicsiss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Macros | Functions
ti_lmk03318.h File Reference

## Macros
#define | TI_LMK03318_FVCO_MAX 5400000000
| Maximum VCO Operating Frequency in Hz. More...
#define | TI_LMK03318_FVCO_MIN 4800000000
| Minimum VCO Operating Frequency in Hz. More...
#define | TI_LMK03318_FOUT_MAX 800000000
| Maximum Output Frequency in Hz. More...
#define | TI_LMK03318_FOUT_MIN 1000000
| Minimum Output Frequency in Hz. More...
#define | TI_LMK03318_FIN_MAX 300000000
| Maximum Input Frequency in Hz. More...
#define | TI_LMK03318_FIN_MIN 1000000
| Minimum Input Frequency in Hz. More...
#define | TI_LMK03318_FPD_MAX 150000000
| Maximum Phase Detector Frequency in Hz. More...
#define | TI_LMK03318_FPD_MIN 1000000
| Minimum Phase Detector Frequency in Hz. More...

## Functions
int | TI_LMK03318_Init (void *IicPtr, u8 I2CSlaveAddress)
| This function initializes the TI LMK03318 with default values for use with the Video FMC. More...
int | TI_LMK03318_PowerDown (void *IicPtr, u8 I2CSlaveAddress)
| This function puts the TI LMK03318 into sleep. More...
int | TI_LMK03318_EnableBypass (void *IicPtr, u8 I2CSlaveAddress, u8 InPortID, u8 OutPortID)
| This function configures the TI LMK03318 to route the specified input port to the specified output port bypassing the PLL. More...
void | TI_LMK03318_RegisterDump (void *IicPtr, u8 I2CSlaveAddress)
| This function displays a registerdump of the TI LMK03318 device. More...