| csi2txss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XCsi2TxSs Struct Reference
Overview

The XCsi2TxSs driver instance data. More...

## Data Fields
XCsi2TxSs_Config | Config
| Hardware configuration. More...
u32 | IsReady
| Device and the driver instance are initialized. More...
XCsi2Tx_SPktData | SpktData
| Short packet. More...

## Detailed Description

The XCsi2TxSs driver instance data.

The user is required to allocate a variable of this type for every XCsi2TxSs device in the system. A pointer to a variable of this type is then passed to the driver API functions.

## Field Documentation

XCsi2TxSs_Config XCsi2TxSs::Config

Hardware configuration.

Referenced by XCsi2TxSs_Activate(), XCsi2TxSs_CfgInitialize(), XCsi2TxSs_Configure(), XCsi2TxSs_GetLineCountForVC(), XCsi2TxSs_IntrDisable(), XCsi2TxSs_ReportCoreInfo(), and XCsi2TxSs_SetLineCountForVC().

u32 XCsi2TxSs::IsReady

Device and the driver instance are initialized.

Referenced by XCsi2TxSs_CfgInitialize(), and XCsi2TxSs_SetCallBack().

XCsi2Tx_SPktData XCsi2TxSs::SpktData

Short packet.

Referenced by XCsi2TxSs_GetShortPacket().