| v_mix Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XV_mix Struct Reference

Driver instance data. More...

## Data Fields
XV_mix_Config | Config
| Hardware Configuration. More...
u32 | IsReady
| Device is initialized and ready. More...

## Detailed Description

Driver instance data.

An instance must be allocated for each core in use.

## Field Documentation

XV_mix_Config XV_mix::Config

Hardware Configuration.

Referenced by XVMix_DbgLayerInfo(), XVMix_DbgReportStatus(), XVMix_GetLayerAlpha(), XVMix_GetLayerBufferAddr(), XVMix_GetLayerChromaBuffer2Addr(), XVMix_GetLayerChromaBufferAddr(), XVMix_GetLayerColorFormat(), XVMix_GetLayerScaleFactor(), XVMix_GetLayerWindow(), XVMix_LoadLogo(), XVMix_LoadLogoPixelAlpha(), XVMix_MoveLayerWindow(), XVMix_SetLayerAlpha(), XVMix_SetLayerBufferAddr(), XVMix_SetLayerChromaBuffer2Addr(), XVMix_SetLayerChromaBufferAddr(), XVMix_SetLayerScaleFactor(), XVMix_SetLayerWindow(), and XVMix_SetVidStream().

u32 XV_mix::IsReady

Device is initialized and ready.

Referenced by XVMix_InterruptHandler().